UNITED PAINT MFG CO/UNITED COATINGS

-- ELASTUFF 504, EF-504-B,PART B -- 5630-00D003554

===================== Product Identification =====================

Product ID:ELASTUFF 504,EF-504-B,PART B

MSDS Date:10/01/1993

FSC:5630

NIIN:00D003554

Kit Part:Y

MSDS Number: BXHRN

=== Responsible Party ===

Company Name:UNITED PAINT MFG CO/UNITED COATINGS

Address:EAST 19011 CATALDO

City:GREENACRES

State:WA

ZIP:99016

Country:US

Info Phone Num:509-926-7143/800-541-4383

Emergency Phone Num:509-926-7143

Preparer's Name:DON LILLY

CAGE:64246

=== Contractor Identification ===

Company Name:UNITED PAINT MFG CO

Address:19011 E CATALDO RD

Box:City:GREENACRES

State:WA

ZIP:99016-5000

Country:US

Phone:509-926-7143/800-835-9673

CAGE:64246

============= Composition/Information on Ingredients =============

Ingred Name:DIETHYLTOLUENEDIAMINE/AROMATIC DIAMINE

CAS:68479-98-1

Fraction by Wt: 100%

Other REC Limits:NONE RECOMMENDED

===================== Hazards Identification =====================

LD50 LC50 Mixture:LD50 (ORAL, RAT) IS 485 MG/KG (TOXIC)

Routes of Entry: Inhalation:NO Skin:YES Ingestion:NO

Reports of Carcinogenicity:NTP:NO IARC:NO OSHA:NO

Health Hazards Acute and Chronic:TARGET ORGANS:EYES, SKIN, GI TRACT.

ACUTE- MAY CAUSE EYE AND SKIN IRRITATION. EXPECTED TO BE TOXIC BY

DERMAL ABSORPTION, DERMAL LD50=700 MG/KG. INHALATION IS NOT

EXPECTED TO BE A ROUTE OF EXPOSURE DUE TO LOW VOLATILITY AT ROOM

TEMPERATURE.EXPECTED TO BE TOXIC BY INGESTION. CHRONIC- PANCREATIC

EFFECTS IN LAB ANIMALS.

Explanation of Carcinogenicity:YNONEINS DICHLOROMETHANE.

Effects of Overexposure:IRRITATION, NAUSEA, VOMITING, ABDOMINAL

DISCOMFORT, HEADACHE

======================= First Aid Measures =======================

First Aid:GET MEDICAL HELP IF SYMPTOMS PERSIST. INHALED:REMOVE TO FRESH

AIR. EYES:FLUSH WITH WATER FOR 15 MINUTES, HOLDING EYELIDS OPEN.

CONSULT A PHYSICIAN. SKIN:REMOVE CONTAMINATED CLOTHING. WASH SKIN

WITH PL ENTY OF SOAP AND WATER. ORAL:IF CONSCIOUS, INDUCE VOMITING.

GET MEDICAL ATTENTION IMMEDIATELY.

===================== Fire Fighting Measures =====================

Flash Point Method:TCC

Flash Point:275F,135C

Extinguishing Media:WATER FOG, CARBON DIOXIDE, SAND, FOAM/DRY CHEMICAL.

WATER SPRAY MAY BE USED TO KEEP FIRE EXPOSED CONTAINERS COOL.

Fire Fighting Procedures:WEAR PROTECTIVE CLOTHING AND NIOSH-APPROVED

SELF-CONTAINED BREATHING APPARATUS. HAZARDOUS DECOMPOSITION

PRODUCTS MAY BE PRESENT.

================== Accidental Release Measures ==================

Spill Release Procedures:WEAR PROTECTIVE EQUIPMENT. STOP LEAK IF

POSSIBLE. ABSORB SPILLS WITH INERT MATERIAL SUCH AS

SAND/VERMICULITE. PLACE IN A SUITABLE CONTAINER FOR LATER DISPOSAL.

WASH SPILL AREA WITH SOAPY WATER AFTER P ICK UP IS COMPLETE.

Neutralizing Agent:NOT RELEVANT

====================== Handling and Storage ======================

Handling and Storage Precautions:STORE IN COOL, DRY, VENTILATED PLACE.

KEEP CONTAINER CLOSED WHEN NOT IN USE.

Other Precautions:DO NOT CUT OR WELD ON EMPTY OR FULL CONTAINERS. WASH

THOROUGHLY AFTER HANDLING AND BEFORE EATING, DRINKING. KEEP OUT OF

REACH OF CHILDREN.

============= Exposure Controls/Personal Protection =============

Respiratory Protection:WEAR NIOSH-APPROVED ORGANIC VAPOR RESPIRATOR IF

MATERIAL IS HEATED.

Ventilation:USE GENERAL OR LOCAL EXHAUST VENTILATION TO KEEP VAPOR

CONCENTRATION AS LOW AS POSSIBLE.

Protective Gloves:NITRILE OR NEOPRENE

Eye Protection:CHEMICAL SPLASH GOGGLES/FACE SHIELD

Other Protective Equipment:EYE WASH STATION, SAFETY SHOWER, PROTECTIVE

CLOTHING

Work Hygienic Practices:OBSERVE GOOD INDUSTRIAL HYGIENE PRACTICES AND

RECOMMENDED PROCEDURES. DO NOT WEAR CONTACT LENSES.

Supplemental Safety and Health

KEY1:T4. THIS PRODUCT IS A KIT CONSISTING OF TWO PARTS. PART A, HAS PNI

A, NSN: 5630-00-D00-3553.

================== Physical/Chemical Properties ==================

HCC:T4

NRC/State Lic Num:NOT RELEVANT

Boiling Pt:B.P. Text:586F,308C

Vapor Pres:10 @ 329F

Vapor Density:<1

Spec Gravity:1.0

Evaporation Rate & Reference:<1 (ETHER=1)

Solubility in Water:MODERATELY SOLUBLE

Appearance and Odor:THIN YELLOW LIQUID - ALCOHOL, KETONE ODOR

================= Stability and Reactivity Data =================

Stability Indicator/Materials to Avoid:YES

NONE

Stability Condition to Avoid:OPEN FLAMES

Hazardous Decomposition Products:CARBON MONOXIDE, CARBON DIOXIDE,

OXIDES OF NITROGEN MAY BE FORMED.

==================== Disposal Considerations ====================

Waste Disposal Methods:DISPOSE OF IN ACCORDANCE WITH ALL LOCAL, STATE

AND FEDERAL REGULATIONS. AVOID CONTAMINATION OF GROUND AND SURFACE

WATER. DO NOT FLUSH TO SEWER.

Disclaimer (provided with this information by the compiling agencies):

This information is formulated for use by elements of the Department

of Defense. The United States of America in no manner whatsoever,

expressly or implied, warrants this information to be accurate and

disclaims all liability for its use. Any person utilizing this

document should seek competent professional advice to verify and

assume responsibility for the suitability of this information to their

particular situation.